| IDA SDK

Macros
Secondary assembler feature bits

## Detailed Description

Used by asm_t::flag2.

## Macros
#define | AS2_BRACE 0x00000001
| Use braces for all expressions.
#define | AS2_STRINV 0x00000002
| Invert meaning of idainfo::wide_high_byte_first for text strings (for processors with bytes bigger than 8 bits)
#define | AS2_BYTE1CHAR 0x00000004
| One symbol per processor byte. More...
#define | AS2_IDEALDSCR 0x00000008
| Description of struc/union is in the 'reverse' form (keyword before name), the same as in borland tasm ideal.
#define | AS2_TERSESTR 0x00000010
| 'terse' structure initialization form; NAME<fld,fld,...> is supported
#define | AS2_COLONSUF 0x00000020
| addresses may have ":xx" suffix; this suffix must be ignored when extracting the address under the cursor
#define | AS2_YWORD 0x00000040
| a_yword field is present and valid
#define | AS2_ZWORD 0x00000080
| a_zword field is present and valid

## Macro Definition Documentation

## ◆ AS2_BYTE1CHAR

#define AS2_BYTE1CHAR 0x00000004

One symbol per processor byte.

Meaningful only for wide byte processors