| IDA SDK

Macros
Register info attribute flags

## Detailed Description

Used by register_info_t::flags.

## Macros
#define | REGISTER_READONLY 0x0001
| the user can't modify the current value of this register
#define | REGISTER_IP 0x0002
| instruction pointer
#define | REGISTER_SP 0x0004
| stack pointer
#define | REGISTER_FP 0x0008
| frame pointer
#define | REGISTER_ADDRESS 0x0010
| may contain an address
#define | REGISTER_CS 0x0020
| code segment
#define | REGISTER_SS 0x0040
| stack segment
#define | REGISTER_NOLF 0x0080
| displays this register without returning to the next line, allowing the next register to be displayed to its right (on the same line)
#define | REGISTER_CUSTFMT 0x0100
| register should be displayed using a custom data format. More...

## Macro Definition Documentation

## ◆ REGISTER_CUSTFMT

#define REGISTER_CUSTFMT 0x0100

register should be displayed using a custom data format.

the format name is in bit_strings[0]; the corresponding regval_t will use bytevec_t