| IDA SDK

Variables
Hardware breakpoint ids

## Detailed Description

Fire the breakpoint upon one of these events.

## Variables
const bpttype_t | BPT_WRITE = 1
| Write access.
const bpttype_t | BPT_READ = 2
| Read access.
const bpttype_t | BPT_RDWR = 3
| Read/write access.
const bpttype_t | BPT_SOFT = 4
| Software breakpoint.
const bpttype_t | BPT_EXEC = 8
| Execute instruction.
const bpttype_t | BPT_DEFAULT = (BPT_SOFT|BPT_EXEC)
| Choose bpt type automatically.