| IDA SDK

Variables
Derived type: array
Type flags

## Detailed Description

For BT_ARRAY, the BTMT_... flags must be equivalent to the BTMT_... flags of its elements

## Variables
const type_t | BT_ARRAY = 0x0B
| array
const type_t | BTMT_NONBASED = 0x10
const type_t | BTMT_ARRESERV = 0x20
| reserved bit

## Variable Documentation

## ◆ BTMT_NONBASED

const type_t BTMT_NONBASED = 0x10

if set
array base==0
format: dt num_elem; [tah-typeattrs]; type_t...
if num_elem==0 then the array size is unknown
else
format: da num_elem, base; [tah-typeattrs]; type_t...

used only for serialization